# ethanol99dnaturvwr

date : 2017-12-30

language_code : en

name : ethanol99dnaturvwr

ph : Not available

## euh_codes

## expositions

code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

## h_codes

H225, H319

## information

## p_codes

P210, P243, P280, P305+P351+P338

## precautions

code: P210 text: P210

code: P243 text: Prendre des mesures de précaution contre les décharges électrostatiques.

code: P280 text: Porter des gants de protection/des vêtements de protection/un équipement de protection des yeux/ du visage.

code: P305+P351+P338 text: EN CAS DE CONTACT AVEC LES YEUX: rincer avec précaution à l’eau pendant plusieurs minutes. Enlever les lentilles de contact si la victime en porte et si elles peuvent être facilement enlevées. Continuer à rincer.

age : 8

## body

skin : Wash the affected area immediately with plenty of water and soap. Remove contaminated, saturated clothing right away. If skin reactions occur, consult a physician.

eyes : Flush the eye immediately with plenty of flowing water for 10–15 minutes while holding the eyelids apart. Remove contact lenses if present and easy to do. Continue rinsing. Consult an ophthalmologist and protect the uninjured eye.

ingestion : If the person is conscious, rinse the mouth with plenty of water. Do **not** induce vomiting. Give nothing to eat or drink. Seek immediate medical attention.

inhalation : Call a POISON CENTRE or a doctor. Move the casualty to fresh air. Keep the person warm and at rest. If breathing is irregular or stopped, give artificial respiration.

## company

name : VWR International Ltd.

## fire

water : True

foam : False

powder : True

co2 : True

other : Nitrogen

## labellings

explosive : False

flammable : True

oxidising : False

gaz : False

corrosive : False

acute : False

health : True

serious : False

hazardous : False

warning : Danger

## protection

skin : **Gloves – short‑term hand contact**: Material: NBR (Nitrile rubber), Thickness: not specified, Breakthrough time (maximum wearing time): 240–480 min. Recommended product: VWR 112‑3717 / VWR 112‑1381. **Gloves – long‑term hand contact**: Material: NBR (Nitrile rubber), Thickness: 0.425 mm, Breakthrough time (maximum wearing time): >480 min. Recommended product: VWR 112‑0971.

eyes : **Eye/face protection**: Eye glasses with side protection, DIN‑/EN‑Norms: DIN EN 166. Recommended product: VWR 111‑0432.

respiratory : **Respiratory protection**: Type: Full-, half- or quarter-face masks, DIN-/EN-Norms: DIN EN 136/140. Material: ABEK2P3. Recommended products: VWR 111-0206 (mask) / VWR 111-0059 (filter).

hands : **Gloves – short‑term hand contact**: Material: NBR (Nitrile rubber), Thickness: not specified, Breakthrough time (maximum wearing time): 240–480 min. Recommended product: VWR 112‑3717 / VWR 112‑1381. **Gloves – long‑term hand contact**: Material: NBR (Nitrile rubber), Thickness: 0.425 mm, Breakthrough time (maximum wearing time): >480 min. Recommended product: VWR 112‑0971.

clothing : **Protective clothing**: Protective clothing with CE-label including the four control digits (no specific material or thickness given). Recommended product: –

## stability

stability : The product is chemically stable under standard ambient conditions (room temperature).

reaction : - Vapours can form explosive mixtures with air. - Potential for explosive mixtures with oxidising agents, nitrogen oxides (NOx), oxygen‑rich materials, nitric acid, chlorine, and bromine. - Exothermic reactions may occur with reducing agents, acids, acid halides, and concentrated alkali. - Violent reactions can occur with alkali metals, alkaline earth metals, and can produce hydrogen.

## state

state : liquid

form : viscous liquid

## storage

safe_handling : - All work processes must be designed so that exposure to inhalation, skin contact, and eye contact is kept as low as possible.
- Use an extractor hood (laboratory).
- If the substance is handled uncovered, arrange for local exhaust ventilation.
- If local exhaust ventilation is not possible or not sufficient, the entire working area must be ventilated by technical means.

safe_storage : - Keep the container tightly closed.
- Store in a well‑ventilated place.
- Store only in the original container.

specific_end_use : Relevant identified uses: General chemical reagent

## transport

ADR : 3

RID : 3

ADN : not available

IMDG : 3

IATA : 3

UN : 1170

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

#### missing_codes

reference_data : None

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

reference_data : None

result : AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

P210 : code: P210 text: P210

P243 : code: P243 text: Prendre des mesures de précaution contre les décharges électrostatiques.

P280 : code: P280 text: Porter des gants de protection/des vêtements de protection/un équipement de protection des yeux/ du visage.

P305+P351+P338 : code: P305+P351+P338 text: EN CAS DE CONTACT AVEC LES YEUX: rincer avec précaution à l’eau pendant plusieurs minutes. Enlever les lentilles de contact si la victime en porte et si elles peuvent être facilement enlevées. Continuer à rincer.

#### missing_codes

reference_data : None

result : AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes : P210, P233, P240, P241, P242, P243, P264, P280, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

Actual Codes : P210, P243, P280, P305+P351+P338

Codes in both sets : P210, P243, P280

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : P233, P240, P241, P242, P264, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

#### missing_codes

P233, P240, P241, P242, P264, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

reference_data : None

result : INVALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

No information available

#### missing_codes

reference_data : None

result : VALID

## Ethanol absolute

cas : 64-17-5

ec : 200-578-6

name : Ethanol absolute

### h_codes

H225, H319

concentrations : strictly greater than 90.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225

Actual Codes : H225, H319

Codes in both sets : H225

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

regulation : REACH Annex XVII (restrictions)

substance : Ethanol absolute

entries : 1

#### missing_codes

result : REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 1000.0

vle-mg-m3 : 1907.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

regulation : RPB

substance : Ethanol absolute

entries : 4

#### missing_codes

result : REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Ethanol absolute

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : FICHENovembre 2019Fiche n°48 - ÉthanolFiche présentant l'essentiel des données d'hygiène et de sécurité relatives à« Éthanol »avec un rappel de la réglementation française et des recommandations techniques et médicales.En savoir plus

url : https://www.inrs.fr/accueil/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_48

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[2, 9, 17-19], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## 2-Propanol

cas : 67-63-0

ec : 200-661-7

name : 2-Propanol

### h_codes

H225, H319, H336

concentrations : greater or equal to 0.5 and less or equal to 2.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225, H319, H336

Actual Codes : H225, H319, H336

Codes in both sets : H225, H319, H336

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

regulation : REACH Annex XVII (restrictions)

substance : 2-Propanol

entries : 1

#### missing_codes

result : REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 200.0

vle-mg-m3 : 500.0

vle-courte-ppm : 400.0

vle-courte-mg-m3 : 1000.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

regulation : RPB

substance : 2-Propanol

entries : 3

#### missing_codes

result : REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : 2-Propanol

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: eye danger: Eye Irrit. text: Provoque une sévère irritation des yeux.

H336 : code: H336 exposition: danger: STOT SE text: Peut provoquer somnolence ou vertiges.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : FICHEJanvier 2021Fiche n°66 - Propan-2-olFiche présentant l'essentiel des données d'hygiène et de sécurité relatives à« Propan-2-ol »avec un rappel de la réglementation française et des recommandations techniques et médicales.En savoir plus

url : https://www.inrs.fr/accueil/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_66

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[16-18], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Methyl ethyl ketone

cas : 78-93-3

ec : 201-159-0

name : Methyl ethyl ketone

### h_codes

H225, H319, H336

concentrations : greater or equal to 0.5 and less or equal to 2.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225, H319, H336

Actual Codes : H225, H319, H336

Codes in both sets : H225, H319, H336

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 200.0

vle-mg-m3 : 600.0

vle-courte-ppm : 300.0

vle-courte-mg-m3 : 900.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Methyl ethyl ketone

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: eye danger: Eye Irrit. text: Provoque une sévère irritation des yeux.

H336 : code: H336 exposition: danger: STOT SE text: Peut provoquer somnolence ou vertiges.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : FICHE2020Fiche n°14 - Butanone ou MéthyléthylcétoneFiche présentant l'essentiel des données d'hygiène et de sécurité relatives à« Butanone ou Méthyléthylcétone »avec un rappel de la réglementation française et des recommandations techniques et médicales.En savoir plus

url : https://www.inrs.fr/accueil/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_14

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[5, 6, 9, 10, 21-23], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED