# ethanolabsolu20821vwr

date : 2017-12-24

language_code : en

name : ethanolabsolu20821vwr

ph : 7

## euh_codes

## expositions

code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

## h_codes

H225, H319

## information

## p_codes

P210, P243, P280, P305+P351+P338, P403+P235

## precautions

code: P210 text: P210

code: P243 text: Prendre des mesures de précaution contre les décharges électrostatiques.

code: P280 text: Porter des gants de protection/des vêtements de protection/un équipement de protection des yeux/ du visage.

code: P305+P351+P338 text: EN CAS DE CONTACT AVEC LES YEUX: rincer avec précaution à l’eau pendant plusieurs minutes. Enlever les lentilles de contact si la victime en porte et si elles peuvent être facilement enlevées. Continuer à rincer.

code: P403+P235 text: Stocker dans un endroit bien ventilé. Tenir au frais.

age : 8

## body

skin : • After contact with skin, wash immediately with plenty of water and soap. • Remove contaminated, saturated clothing immediately. • If skin reactions occur, consult a physician.

eyes : • Flush immediately with plenty of flowing water for 10–15 minutes while holding the eyelids apart. • Remove contact lenses if present and easy to do. • Continue rinsing. • Consult an ophthalmologist and protect the uninjured eye.

ingestion : • If accidentally swallowed, rinse the mouth with plenty of water (only if the person is conscious). • Obtain immediate medical attention. • Do NOT induce vomiting. • Give nothing to eat or drink.

inhalation : • Call a POISON CENTRE or a doctor. • Remove the casualty to fresh air and keep warm and at rest. • If breathing is irregular or stopped, administer artificial respiration.

## company

name : VWR International Ltd.

## fire

water : True

foam : False

powder : True

co2 : True

other : Nitrogen

## labellings

explosive : False

flammable : True

oxidising : False

gaz : False

corrosive : False

acute : False

health : True

serious : False

hazardous : False

warning : Danger

## protection

skin : Wear nitrile gloves (NBR) with the specified breakthrough times and recommended articles for both short‑ and long‑term hand contact. • Thickness: not specified480 min

eyes : Use eye glasses that meet DIN‑EN 166 with side protection (VWR 111‑0432). • Eye glasses with side protection, DIN‑EN 166 standard

respiratory : If aerosol or mist is generated, use a full‑, half‑, or quarter‑face mask (DIN EN 136/140) with ABEK2P3 filter material (VWR 111‑0206). • Full‑face, half‑face, or quarter‑face masks (DIN EN 136/140)

hands : Wear nitrile gloves (NBR) with the specified breakthrough times and recommended articles for both short‑ and long‑term hand contact. • Thickness: not specified480 min

clothing : Wear protective clothing that carries a CE‑label with the four control digits; specific material or thickness is not detailed. • Must have CE‑label including the four control digits

## stability

stability : The product is chemically stable under standard ambient conditions (room temperature).

reaction : No data available.

## state

state : liquid

form : -

## storage

safe_handling : **Precautions for safe handling** 1. **General work‑process precautions**
- Design work processes so that inhalation, skin contact, and eye contact are kept as low as possible.
- Keep away from sources of ignition: no smoking, no open flames, no sparks, no hot surfaces.
- Take precautionary measures against static discharges.
- Protect from moisture.

2. **Personal protective equipment (PPE)**
   - **Protective clothing**: wear suitable protective clothing with CE‑label including the four control digits.
   - **Eye/face protection**: eye glasses with side protection (DIN EN 166).
   - **Skin protection**:
   - For short‑term hand contact: NBR (nitrile rubber) gloves, breakthrough time 240‑480 min, recommended articles VWR 112‑3717 / 112‑1381.
   - For long‑term hand contact: NBR gloves, thickness 0.425 mm, breakthrough time > 480 min, recommended article VWR 112‑0971.
   - **Respiratory protection** (if aerosol or mist formation): full‑, half‑, or quarter‑face masks (DIN EN 136/140), recommendation VWR 111‑0206, suitable material ABEK2P3 (VWR 111‑0059).

3. **Engineering controls**
   - Use local exhaust ventilation when handling uncovered.

4. **Other safety measures**
   - Provide an eye shower and label its location conspicuously.
   - Wash hands before breaks and after work.
   - Avoid contact with skin and eyes; do not eat, drink, or smoke while handling.

safe_storage : **Conditions for safe storage (including incompatibilities)** - **Recommended storage temperature:** 15 – 25 °C - **Storage class:** 3 - **Container handling:** Keep the container tightly closed and in a well‑ventilated place. - **Location:** Store away from combustible materials.

**Incompatibilities:** No specific incompatibilities are listed in the document.

specific_end_use : **Intended use:** General chemical reagent.

## transport

ADR : 3

RID : 3

ADN : not available

IMDG : 3

IATA : 3

UN : 1170

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

#### missing_codes

reference_data : None

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

reference_data : None

result : AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

P210 : code: P210 text: P210

P243 : code: P243 text: Prendre des mesures de précaution contre les décharges électrostatiques.

P280 : code: P280 text: Porter des gants de protection/des vêtements de protection/un équipement de protection des yeux/ du visage.

P305+P351+P338 : code: P305+P351+P338 text: EN CAS DE CONTACT AVEC LES YEUX: rincer avec précaution à l’eau pendant plusieurs minutes. Enlever les lentilles de contact si la victime en porte et si elles peuvent être facilement enlevées. Continuer à rincer.

P403+P235 : code: P403+P235 text: Stocker dans un endroit bien ventilé. Tenir au frais.

#### missing_codes

reference_data : None

result : AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes : P210, P233, P240, P241, P242, P243, P264, P280, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

Actual Codes : P210, P243, P280, P305+P351+P338, P403+P235

Codes in both sets : P210, P243, P280

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : P233, P240, P241, P242, P264, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

#### missing_codes

P233, P240, P241, P242, P264, P303 + P361 + P353, P305 + P351 + P338, P337 + P313, P370 + P378, P403 + P235, P501

reference_data : None

result : INVALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

No information available

#### missing_codes

reference_data : None

result : VALID

## Ethanol absolute

cas : 64-17-5

name : Ethanol absolute

### h_codes

H225, H319

concentrations : strictly greater than 0.0 and strictly less than 0.0

ec : None

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225

Actual Codes : H225, H319

Codes in both sets : H225

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

regulation : REACH Annex XVII (restrictions)

substance : Ethanol absolute

entries : 1

#### missing_codes

result : REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 1000.0

vle-mg-m3 : 1907.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

regulation : RPB

substance : Ethanol absolute

entries : 4

#### missing_codes

result : REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Ethanol absolute

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : FICHENovembre 2019Fiche n°48 - ÉthanolFiche présentant l'essentiel des données d'hygiène et de sécurité relatives à« Éthanol »avec un rappel de la réglementation française et des recommandations techniques et médicales.En savoir plus

url : https://www.inrs.fr/accueil/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_48

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[2, 9, 17-19], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED