# n27co2bonbonne

date : 2022-01-01

language_code : en

name : n27co2bonbonne

ph : Not available

## euh_codes

## expositions

code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

## h_codes

H280

## information

## p_codes

P403

## precautions

code: P403 text: Stocker dans un endroit bien ventilé.

age : 4

## body

skin : • In case of frostbite, spray the affected area with water for at least 15 minutes. • Apply a sterile dressing. • Obtain medical assistance.

eyes : • Immediately flush the eyes thoroughly with water for at least 15 minutes.

ingestion : • Ingestion is not considered a potential route of exposure. (No specific first‑aid action required.)

inhalation : • Remove the victim to an uncontaminated area wearing a self‑contained breathing apparatus. • Keep the victim warm and rested. • Call a doctor. • Perform cardiopulmonary resuscitation if breathing stops.

## company

name : AIR LIQUIDE BeNeLux

## fire

water : True

foam : False

powder : False

co2 : False

other : -

## labellings

explosive : False

flammable : False

oxidising : False

gaz : True

corrosive : False

acute : False

health : False

serious : False

hazardous : False

warning : Attention

## protection

skin : Working gloves \| **EN 388 – Protective gloves against mechanical risk, performance level 1 or higher** \| • Minimum abrasion resistance (level 1).

Cold‑insulating gloves \| **EN 511 – Cold insulating gloves** \| • Designed for protection against cold burns/frostbite when handling liquid CO₂.

eyes : Safety goggles \| **EN 166 – Personal eye‑protection – specifications** \| • Full‑face coverage, impact‑resistant lenses.

respiratory : Self‑contained breathing apparatus (SCBA) \| **EN 137 – Self‑contained open‑circuit compressed air breathing apparatus with full face mask** \| • Provides a safe breathing environment in oxygen‑deficient atmospheres.

Positive‑pressure airline with mask (alternative) \| – \| • Used when SCBA is not available; provides positive‑pressure protection against gas ingress.

hands : Working gloves \| **EN 388 – Protective gloves against mechanical risk, performance level 1 or higher** \| • Minimum abrasion resistance (level 1).

Cold‑insulating gloves \| **EN 511 – Cold insulating gloves** \| • Designed for protection against cold burns/frostbite when handling liquid CO₂.

clothing : -

## stability

stability : Stable under normal conditions

reaction : No reactivity hazard other than the effects described in the sub‑sections below.

## state

state : Gas

form : Not specified as a fine powder, powder, grains, granules, pellets, viscous liquid, or paste.

## storage

safe_handling : - Do not breathe the gas. - Avoid release of the product into the work area. - Handle the gas only with good industrial hygiene and safety procedures. - Only experienced and properly instructed persons should handle gases under pressure. - Consider pressure‑relief device(s) in gas installations. - Ensure the complete gas system is (or is regularly) checked for leaks before use. - Do not smoke while handling the product. - Use only properly specified equipment which is suitable for this product, its supply pressure and temperature. - Contact your gas supplier if in doubt. - Avoid suck‑back of water, acid and alkalis. - Containers that have contained flammable or explosive substances must not be inerted with liquid CO₂; potential production of solid CO₂ particles must be ruled out. - Ensure the system is adequately grounded to avoid electrostatic discharge. - Be aware of the risk of static electricity with CO₂ extinguishers; do not use them where a flammable atmosphere may be present. - Protect containers from physical damage; do not drag, roll, slide or drop them. - Do not allow back‑feed into the container. - When moving cylinders, use a cart (trolley, hand truck, etc.) designed to transport cylinders. - Leave valve protection caps in place until the container has been secured against a wall, bench or placed in a container stand and is ready for use. - If you experience difficulty operating the valve, discontinue use and contact the supplier. - Never attempt to repair or modify container valves or safety‑relief devices. - Report damaged valves immediately to the supplier. - Keep container valve outlets clean and free from contaminants, especially oil and water. - Replace valve outlet caps or plugs and container caps where supplied as soon as the container is disconnected from equipment. - Close the container valve after each use and when empty, even if still connected to equipment. - Never attempt to transfer gases from one cylinder/container to another. - Never use direct flame or electrical heating devices to raise the pressure of a container. - Do not remove or deface labels provided by the supplier for the identification of the content of the container. - Prevent suck‑back of water into the container. - Open the valve slowly to avoid pressure shock. - Keep containers stored in the vertical position and properly secured to prevent them from falling over.

safe_storage : - Observe all regulations and local requirements for storing containers. - Do not store containers in conditions that could encourage corrosion. - Keep valve guards or caps in place. - Store containers in the vertical position and secure them to prevent falling. - Periodically check containers for general condition and leakage. - Keep containers below 50 °C in a well‑ventilated place. - Store containers in a location free from fire risk and away from sources of heat and ignition. - Keep containers away from combustible materials. **Potential incompatibilities** - Containers that have contained flammable or explosive substances must not be inerted with liquid CO₂; solid CO₂ particles must be ruled out. - For detailed compatibility information, refer to ISO 11114.

specific_end_use : - Industrial and professional uses (perform risk assessment prior to use). - Test gas / Calibration gas. - Purge gas, diluting gas, inerting gas. - Purging. - Shield gas for welding processes. - Use for manufacture of electronic/photovoltaic components. - Laboratory and process control.

## transport

ADR : 2

RID : 2

ADN : not available

IMDG : 2.2

IATA : 2.2

UN : 1013

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H280 : code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

#### missing_codes

reference_data : None

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04

signal_word : Warning

#### missing_codes

reference_data : None

result : AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

P403 : code: P403 text: Stocker dans un endroit bien ventilé.

#### missing_codes

reference_data : None

result : AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes : P410 + P403

Actual Codes : P403

Codes in both sets :

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : P410 + P403

#### missing_codes

P410 + P403

reference_data : None

result : INVALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

No information available

#### missing_codes

reference_data : None

result : VALID

## Carbon dioxide

cas : 124-38-9

ec : 204-696-9

name : Carbon dioxide

### h_codes

H280

concentrations : greater or equal to 100.0 and less or equal to 100.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H280

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 5000.0

vle-mg-m3 : 9131.0

vle-courte-ppm : 30000.0

vle-courte-mg-m3 : 54784.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

regulation : RPB

substance : Carbon dioxide

entries : 4

#### missing_codes

result : REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H280 : code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04

signal_word : Warning

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : FICHEJuin 2020Fiche n°238 - Dioxyde de carboneFiche présentant l'essentiel des données d'hygiène et de sécurité relatives à« Dioxyde de carbone »avec un rappel de la réglementation française et des recommandations techniques et médicales.En savoir plus

url : https://www.inrs.fr/accueil/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_238

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion, Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED