# certified-np1aerosolgrez

date : 2019-01-21

language_code : fr

name : certified-np1aerosolgrez

ph : Non disponible

## euh_codes

EUH066

## expositions

code: H222 exposition: danger: ▼M4 text: Aérosol extrêmement inflammable.

code: H229 exposition: danger: ▼M4 text: Pressurised container: May burst if heated

code: H315 exposition: danger: 3.2.4.

Hazard Communication text: Provoque une irritation cutanée.

code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

code: H411 exposition: danger: 4.1.4. Hazard communication text: Toxique pour les organismes aquatiques, entraîne des effets néfastes à long terme.

code: EUH066 exposition: danger: text: L'exposition répétée peut provoquer dessèchement ou gerçures de la peau.

## h_codes

H222, H229, H315, H336, H411

## information

## p_codes

P210, P211, P251, P260, P271, P273, P302+P352, P312, P391, P410+P412

## precautions

code: P210 text: P210

code: P211 text: Ne pas vaporiser sur une flamme nue ou sur toute autre source d’ignition.

code: P251 text: P251

code: P260 text: Ne pas respirer les poussières/fumées/gaz/brouillards/vapeurs/ aérosols.

code: P271 text: Utiliser seulement en plein air ou dans un endroit bien ventilé.

code: P273 text: Éviter le rejet dans l’environnement.

code: P302+P352 text: EN CAS DE CONTACT AVEC LA PEAU:

code: P312 text: P312

code: P391 text: Recueillir le produit répandu.

code: P410+P412 text: Protéger du rayonnement solaire.

age : 7

## body

skin : **Contact avec la peau** • Laver immédiatement et abondamment avec de l’eau et du savon. • Enlever les vêtements contaminés et les chaussures. • Faire appel à une assistance médicale en cas d’apparition d’une irritation qui persiste.

eyes : **Contact avec les yeux** • Rincer immédiatement avec beaucoup d’eau pendant au moins 15 minutes. • Faire appel à une assistance médicale en cas d’apparition d’une irritation qui persiste.

ingestion : **Ingestion** • Se rincer la bouche à l’eau. • En cas d’ingestion, ne pas faire vomir – consulter un médecin.

inhalation : **Inhalation** • Si les troubles se prolongent, consulter un médecin. • En cas d’exposition à de fortes concentrations d’aérosols, aller à l’air libre.

## company

name : NCH Belgium Inc.

## fire

water : True

foam : True

powder : True

co2 : True

other : -

## labellings

explosive : False

flammable : True

oxidising : False

gaz : False

corrosive : False

acute : False

health : True

serious : False

hazardous : False

warning : Danger

## protection

skin : - Gants résistants aux solvants (caoutchouc butyle). - Caoutchouc fluoré. - Alcool de polyvinyle.

eyes : - Lunettes de sécurité approuvées selon la norme EN 166.

respiratory : - Masques ou respirateurs à filtre adapté aux vapeurs organiques. Le texte indique que, lorsqu’une ventilation insuffisante est présente, il faut porter un équipement de protection respiratoire. Les masques doivent être conformes à la norme EN 14387 (vapeurs organiques).

hands : - Gants de protection conformes à la norme EN 374.

clothing : -

## stability

stability : Il est stable dans des conditions normales.

reaction : Le mélange ne réagira pas dangereusement ni ne polymérisera dans les conditions normales d’utilisation. A haute température, le mélange peut émettre du monoxyde ou du dioxyde de carbone, des fumées ou des oxydes d’azote.

## state

state : liquide

form : liquide visqueux

## storage

safe_handling : - Éviter de respirer les vapeurs ou le brouillard. - Ne pas manger, boire ou fumer en manipulant ce produit. - Tenir à l’abri des flammes nues, des surfaces chaudes et des sources d’inflammation. - Éviter l’accumulation de charges électrostatiques. - Assurer une ventilation adéquate.

safe_storage : - Tenir à l’écart de la chaleur et des sources d’ignition. - Stocker conformément à la réglementation locale. - Pour des raisons de sécurité en cas d’incendie, les bidons doivent être entreposés séparément, dans des enceintes fermées. - Récipient sous pression. - Protéger contre les rayons solaires et ne pas exposer à une température supérieure à 50 °C. - Éviter la chaleur, les flammes et les étincelles.

**Incompatibilités potentielles** - Oxydants forts.

specific_end_use : Lubrifiant et Protecteur

## transport

ADR : Classe de danger 2.1

RID : Classe de danger 2.1

ADN : pas disponible

IMDG : Classe de danger 2.1

IATA : Classe de danger 2.1

UN : UN1950

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H222 : code: H222 exposition: danger: ▼M4 text: Aérosol extrêmement inflammable.

H229 : code: H229 exposition: danger: ▼M4 text: Pressurised container: May burst if heated

H315 : code: H315 exposition: danger: 3.2.4.

Hazard Communication text: Provoque une irritation cutanée.

H336 : code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

H411 : code: H411 exposition: danger: 4.1.4. Hazard communication text: Toxique pour les organismes aquatiques, entraîne des effets néfastes à long terme.

EUH066 : code: EUH066 exposition: danger: text: L'exposition répétée peut provoquer dessèchement ou gerçures de la peau.

#### missing_codes

reference_data : None

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS07, GHS02

signal_word : Danger

#### missing_codes

reference_data : None

result : AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

P210 : code: P210 text: P210

P211 : code: P211 text: Ne pas vaporiser sur une flamme nue ou sur toute autre source d’ignition.

P251 : code: P251 text: P251

P260 : code: P260 text: Ne pas respirer les poussières/fumées/gaz/brouillards/vapeurs/ aérosols.

P271 : code: P271 text: Utiliser seulement en plein air ou dans un endroit bien ventilé.

P273 : code: P273 text: Éviter le rejet dans l’environnement.

P302+P352 : code: P302+P352 text: EN CAS DE CONTACT AVEC LA PEAU:

P312 : code: P312 text: P312

P391 : code: P391 text: Recueillir le produit répandu.

P410+P412 : code: P410+P412 text: Protéger du rayonnement solaire.

#### missing_codes

reference_data : None

result : AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes : P210, P211, P251, P261, P264, P271, P280, P302 + P352, P304 + P340, P312, P321, P332 + P313, P362 + P364, P403 + P233, P405, P410 + P412, P501

Actual Codes : P210, P211, P251, P260, P271, P273, P302+P352, P312, P391, P410+P412

Codes in both sets : P210, P211, P251, P271, P312

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : P261, P264, P280, P302 + P352, P304 + P340, P321, P332 + P313, P362 + P364, P403 + P233, P405, P410 + P412, P501

#### missing_codes

P261, P264, P280, P302 + P352, P304 + P340, P321, P332 + P313, P362 + P364, P403 + P233, P405, P410 + P412, P501

reference_data : None

result : INVALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

No information available

#### missing_codes

reference_data : None

result : VALID

## HYDROCARBONS, C7, N-ALKANES, ISOALKANES, CYCLICS

cas : 64742-49-0

ec : 927-510-4

name : HYDROCARBONS, C7, N-ALKANES, ISOALKANES, CYCLICS

### h_codes

H225, H304, H315, H336, H411

concentrations : greater or equal to 50.0 and strictly less than 100.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H225, H304, H315, H336, H411

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : HYDROCARBONS, C7, N-ALKANES, ISOALKANES, CYCLICS

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

regulation : SEVESO

substance : HYDROCARBONS, C7, N-ALKANES, ISOALKANES, CYCLICS

h_code : H411

###### categories

code : E2

section : E

label : E2 Danger pour l'environnement aquatique dans la catégorie chronique 2

threshold_low : 200.0

threshold_high : 500.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

H304 : code: H304 exposition: danger: Asp. Tox. text: Peut être mortel en cas d’ingestion et de pénétration dans les voies respiratoires.

H315 : code: H315 exposition: danger: 3.2.4.

Hazard Communication text: Provoque une irritation cutanée.

H336 : code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

H411 : code: H411 exposition: danger: 4.1.4. Hazard communication text: Toxique pour les organismes aquatiques, entraîne des effets néfastes à long terme.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS08

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°322 - Solvants aliphatiques en C5-C9

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_322

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[10-12], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## PETROLATUM (PETROLEUM) CLAY-TREATED

cas : 100684-33-1

ec : 309-706-6

name : PETROLATUM (PETROLEUM) CLAY-TREATED

### h_codes

concentrations : greater or equal to 10.0 and strictly less than 20.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes :

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

No information available

#### missing_codes

result : NOT_AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS08

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for PETROLATUM (PETROLEUM) CLAY-TREATED

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## PROPANE

cas : 74-98-6

ec : 200-827-9

name : PROPANE

### h_codes

H220

concentrations : greater or equal to 10.0 and strictly less than 20.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H220

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 1000.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : PROPANE

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for PROPANE

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## BUTANE

cas : 106-97-8

ec : 203-448-7

name : BUTANE

### h_codes

H220

concentrations : greater or equal to 10.0 and strictly less than 20.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H220

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-courte-ppm : 980.0

vle-courte-mg-m3 : 2370.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : BUTANE

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for BUTANE

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED