# motipindustrialcoatingsralcolors400ml

date : 2021-12-10

language_code : fr

name : motipindustrialcoatingsralcolors400ml

ph : Non disponible

## euh_codes

EUH066, EUH211

## expositions

code: H229 exposition: danger: ▼M4 text: Pressurised container: May burst if heated

code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

## h_codes

H222, H229, H319, H336

## information

## p_codes

P101, P102, P210, P211, P251, P260, P410+P412, P501

## precautions

code: P101 text: En cas de consultation d’un médecin, garder à disposition le récipient ou l’étiquette.

code: P102 text: Tenir hors de portée des enfants.

code: P210 text: P210

code: P211 text: Ne pas vaporiser sur une flamme nue ou sur toute autre source d’ignition.

code: P251 text: P251

code: P260 text: Ne pas respirer les poussières/fumées/gaz/brouillards/vapeurs/ aérosols.

code: P410+P412 text: Protéger du rayonnement solaire.

code: P501 text: Éliminer le contenu/récipient dans …

age : 4

## body

skin : - En règle générale, le produit n’irrite pas la peau.

eyes : - Rincer les yeux pendant plusieurs minutes sous l’eau courante en écartant bien les paupières. - Si les troubles persistent, consulter un médecin.

ingestion : - Boire de l’eau en abondance. - Donner de l’air frais. - Consulter immédiatement un médecin.

inhalation : - Donner de l’air frais. - Consulter un médecin en cas de troubles.

## company

name : European Aerosols GmbH

## fire

water : True

foam : False

powder : True

co2 : True

other : Mousse résistante à l’alcool (pour les foyers importants)

## labellings

explosive : False

flammable : True

oxidising : False

gaz : False

corrosive : False

acute : False

health : True

serious : False

hazardous : False

warning : Danger

## protection

skin : **Gants de protection** \| • Matériau : caoutchouc butyle (butylcaoutchouc)

eyes : **Lunettes / écrans faciaux** \| • Type : lunettes de protection hermétiques (écrans faciaux non spécifiés, mais mentionnées comme « Lunettes de protection hermétique

respiratory : **Masques / filtres respiratoires** \| • Filtre : A2/P3 (filtre à particules et à gaz)

hands : **Gants de protection** \| • Matériau : caoutchouc butyle (butylcaoutchouc)

clothing : **Vêtements de protection** \| • Type : vêtement de protection léger (combinaison ou tenue de protection légère).

## stability

stability : Pas de décomposition thermique en cas d’usage conforme. Aucune réaction dangereuse connue. Pas de produits de décomposition dangereux connus.

reaction : Aucune réaction dangereuse connue.

## state

state : aérosol

form : aérosol

## storage

safe_handling : - Protéger de la forte chaleur et du rayonnement direct du soleil. - Veiller à une bonne aération du local, même au niveau du sol (les vapeurs sont plus lourdes que l’air). - Veiller à une bonne ventilation/aspiration du poste de travail. - Ne pas vaporiser vers une flamme ou un corps incandescent. - Tenir à l’abri des sources d’inflammation – ne pas fumer. - Tenir des appareils de protection respiratoire prêts.

safe_storage : - Respecter les prescriptions légales pour le stockage des emballages sous pression. - Tenir les emballages hermétiquement fermés. - Classe de stockage : 2 B.

specific_end_use : **Utilisation prévue:** - Utilisation par des consommateurs : ménages privés / public général / consommateurs - Utilisation professionnelle : domaine public (administration, éducation, spectacle, services, artisans)

## transport

ADR : Classe 2 5F (Gaz) – Étiquette 2.1

RID : - pas disponible

ADN : - pas disponible

IMDG : Classe 2.1 (Gaz) – Label 2.1

IATA : Classe 2.1 (Gaz) – Label 2.1

UN : UN1950

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H229 : code: H229 exposition: danger: ▼M4 text: Pressurised container: May burst if heated

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

H336 : code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

#### missing_codes

reference_data : None

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

reference_data : None

result : AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

P101 : code: P101 text: En cas de consultation d’un médecin, garder à disposition le récipient ou l’étiquette.

P102 : code: P102 text: Tenir hors de portée des enfants.

P210 : code: P210 text: P210

P211 : code: P211 text: Ne pas vaporiser sur une flamme nue ou sur toute autre source d’ignition.

P251 : code: P251 text: P251

P260 : code: P260 text: Ne pas respirer les poussières/fumées/gaz/brouillards/vapeurs/ aérosols.

P410+P412 : code: P410+P412 text: Protéger du rayonnement solaire.

P501 : code: P501 text: Éliminer le contenu/récipient dans …

#### missing_codes

reference_data : None

result : AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes : P210, P211, P251, P261, P264, P271, P280, P304 + P340, P305 + P351 + P338, P312, P337 + P313, P403 + P233, P405, P410 + P412, P501

Actual Codes : P101, P102, P210, P211, P251, P260, P410+P412, P501

Codes in both sets : P210, P211, P251, P501

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : P261, P264, P271, P280, P304 + P340, P305 + P351 + P338, P312, P337 + P313, P403 + P233, P405, P410 + P412

#### missing_codes

P261, P264, P271, P280, P304 + P340, P305 + P351 + P338, P312, P337 + P313, P403 + P233, P405, P410 + P412

reference_data : None

result : INVALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

reason : Si une substance a une classification H351 et est présente à une concentration >= 0,1 %, le produit doit être classé H351 (Cancérogène).

substance_name : Dioxyde de titane

substance_classification : H351

substance_concentration : None–2.5%

rule_threshold : 0.1%

classification : Le produit doit avoir la classification supplémentaire ['H351'].

#### missing_codes

H351

reference_data : None

result : INVALID

## Acétone

cas : 67-64-1

ec : 200-662-2

name : Acétone

### h_codes

H225, H319, H336

concentrations : greater or equal to 25.0 and strictly less than 50.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225, H319, H336

Actual Codes : H225, H319, H336

Codes in both sets : H225, H319, H336

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 246.0

vle-mg-m3 : 594.0

vle-courte-ppm : 492.0

vle-courte-mg-m3 : 1187.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Acétone

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: eye danger: Eye Irrit. text: Provoque une sévère irritation des yeux.

H336 : code: H336 exposition: danger: STOT SE text: Peut provoquer somnolence ou vertiges.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°3 - Acétone

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_3

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[1-3, 26-28], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Acétate de n-butyle

cas : 123-86-4

ec : 204-658-1

name : Acétate de n-butyle

### h_codes

H226, H336

concentrations : greater or equal to 12.5 and strictly less than 20.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H226, H336

Actual Codes : H226, H336

Codes in both sets : H226, H336

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 50.0

vle-mg-m3 : 238.0

vle-courte-ppm : 150.0

vle-courte-mg-m3 : 712.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Acétate de n-butyle

h_code : H226

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H226 : code: H226 exposition: danger: Flam. Liq. text: Liquide et vapeurs inflammables.

H336 : code: H336 exposition: danger: STOT SE text: Peut provoquer somnolence ou vertiges.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07

signal_word : Warning

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°31 - Acétate de n-butyle

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_31

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[3, 6], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Propane

cas : 74-98-6

ec : 200-827-9

name : Propane

### h_codes

H220, H280

concentrations : greater or equal to 10.0 and strictly less than 12.5

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H220

Actual Codes : H220, H280

Codes in both sets : H220

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 1000.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Propane

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

H280 : code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Propane

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Butane

cas : 106-97-8

ec : 203-448-7

name : Butane

### h_codes

H220

concentrations : greater or equal to 5.0 and strictly less than 10.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H220

Actual Codes : H220

Codes in both sets : H220

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-courte-ppm : 980.0

vle-courte-mg-m3 : 2370.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Butane

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Butane

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Acétate de 2-méthoxy-1-méthyléthyle

cas : 108-65-6

ec : 203-603-9

name : Acétate de 2-méthoxy-1-méthyléthyle

### h_codes

H226, H336

concentrations : greater or equal to 5.0 and strictly less than 10.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H226

Actual Codes : H226, H336

Codes in both sets : H226

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 50.0

vle-mg-m3 : 275.0

vle-courte-ppm : 100.0

vle-courte-mg-m3 : 550.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Acétate de 2-méthoxy-1-méthyléthyle

h_code : H226

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H226 : code: H226 exposition: danger: Flam. Liq. text: Liquide et vapeurs inflammables.

H336 : code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02

signal_word : Warning

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°221 - 1-Méthoxy-2-propanol et son acétate

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_221

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[1, 2, 14], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Isobutane

cas : 75-28-5

ec : 200-857-2

name : Isobutane

### h_codes

H220, H280

concentrations : greater or equal to 2.5 and strictly less than 5.0

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H220

Actual Codes : H220, H280

Codes in both sets : H220

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-courte-ppm : 980.0

vle-courte-mg-m3 : 2370.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Isobutane

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

H280 : code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Isobutane

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Nitrate de cellulose

cas : 9004-70-0

name : Nitrate de cellulose

### h_codes

H228

concentrations : greater or equal to 2.5 and strictly less than 5.0

ec : None

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H228

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H228 : code: H228 exposition: danger: Label elements for flammable solids text: Matière solide inflammable.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS01

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Nitrate de cellulose

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Xylène

ec : 905-588-0

name : Xylène

### h_codes

H226, H304, H312, H315, H319, H332, H335, H373

cas : None

concentrations : strictly less than 2.5

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H226, H304, H312, H315, H319, H332, H335, H373

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Xylène

h_code : H226

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H226 : code: H226 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs inflammables.

H304 : code: H304 exposition: danger: Aspiration toxicity label elements text: Peut être mortel en cas d’ingestion et de pénétration dans les voies respiratoires.

H312 : code: H312 exposition: dermal danger: Acute toxicity label elements text: Nocif par contact cutané.

H315 : code: H315 exposition: danger: 3.2.4.

Hazard Communication text: Provoque une irritation cutanée.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

H332 : code: H332 exposition: inhalation danger: Acute toxicity label elements text: Nocif par inhalation.

H373 : code: H373 exposition: danger: Label elements for specific target organ toxicity after repeated exposure text: Risque présumé d'effets graves pour les organes à la suite d'expositions répétées ou d'une exposition prolongée.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02, GHS07, GHS08

signal_word : Warning

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Xylène

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Dioxyde de titane

cas : 13463-67-7

ec : 236-675-5

name : Dioxyde de titane

### h_codes

H351

concentrations : strictly less than 2.5

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes : H351

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-mg-m3 : 10.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H351 : code: H351 exposition: danger: Label elements for carcinogenicity text: Susceptible de provoquer le cancer.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS08

signal_word : Warning

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°291 - Dioxyde de titane

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_291

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[5, 15, 16], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

regulation : CMR

substance : Dioxyde de titane

h_code : H351

#### missing_codes

result : REGULATED

## Éthanol

cas : 64-17-5

ec : 200-578-6

name : Éthanol

### h_codes

H225, H319

concentrations : strictly less than 2.5

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H225

Actual Codes : H225, H319

Codes in both sets : H225

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

regulation : REACH Annex XVII (restrictions)

substance : Éthanol

entries : 1

#### missing_codes

result : REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-ppm : 1000.0

vle-mg-m3 : 1907.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

regulation : RPB

substance : Éthanol

entries : 4

#### missing_codes

result : REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Éthanol

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Flam. Liq. text: Liquide et vapeurs très inflammables.

H319 : code: H319 exposition: danger: 3.3.4.

Hazard Communication text: Provoque une sévère irritation des yeux.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°48 - Éthanol

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_48

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[2, 9, 17-19], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED