# 3m-aerosolscotch1609tubok

date : 2016-05-17

language_code : fr

name : 3m-aerosolscotch1609tubok

ph : Non disponible

## euh_codes

## expositions

## h_codes

## information

## p_codes

## precautions

age : 9

## body

skin : Rincer la peau gelée avec de l’eau tiède. Ne pas frotter la zone affectée. Consulter un médecin.

eyes : Rincer immédiatement avec beaucoup d’eau. Enlever les lentilles de contact si la victime en porte et si elles peuvent être facilement enlevées. Continuer à rincer. Consulter un médecin.

ingestion : Rincer la bouche. En cas de malaise, consulter un médecin.

inhalation : Transporter la personne à l’air frais. Consulter un médecin.

## company

name : 3M France

## fire

water : False

foam : False

powder : False

co2 : True

other : -

## labellings

explosive : False

flammable : False

oxidising : False

gaz : False

corrosive : False

acute : False

health : False

serious : False

hazardous : False

warning : Not Applicable

## protection

skin : -

eyes : **Protection des yeux / du visage** • Écran total.

respiratory : **Masques respiratoires / filtres** • Demi‑masque respiratoire ou masque complet pour vapeurs organiques.

hands : **Gants / protection de la peau / des mains** • Matériau : caoutchouc nitrile.

clothing : **Vêtements de protection / combinaisons** – Aucun vêtement ou combinaison spécifique n’est mentionné dans la section 8.

## stability

stability : stable

reaction : Le produit peut être réactif avec certains agents sous certaines conditions

## state

state : liquide

form : aerosol (en suspension dans l’air)

## storage

safe_handling : **Précautions à prendre pour une manipulation sans danger :** - Éviter l’inhalation des vapeurs pendant la polymérisation.
- Ne pas utiliser en espace confiné ou insuffisamment aéré.
- Tenir hors de portée des enfants.
- Tenir à l’écart de la chaleur, des étincelles, des flammes nues et des surfaces chaudes.
- Ne pas fumer.
- Ne pas vaporiser sur une flamme nue ou sur toute autre source d’ignition.
- Récipient sous pression : ne pas perforer, ni brûler, même après usage.
- Ne pas respirer les poussières, fumées, gaz, brouillards, vapeurs, aérosols.
- Éviter tout contact avec les yeux, la peau ou les vêtements.
- Ne pas manger, ne pas boire et ne pas fumer pendant l’utilisation.
- Se laver soigneusement après manipulation.
- Éviter tout contact avec des agents oxydants (par ex. chlore, l’acide chromique, etc.).

safe_storage : Stocker dans un endroit bien ventilé.
Maintenir le récipient fermé de manière étanche.
Protéger du rayonnement solaire.
Ne pas exposer à une température supérieure à 50 °C / 122 °F.
Stocker à l’écart de la chaleur.
Stocker à l’écart des acides.
Stocker à l’écart des agents oxydants.

specific_end_use : Lubrifiant Silicone

## transport

ADR : classe 5F

RID : classe 5F

ADN : pas disponible

IMDG : classe 2.1

IATA : classe 2.1

UN : UN1950

## Validations

### Product

name : Product

role : Check if the product is compliant with all the validators

#### information

No information available

#### missing_codes

overall_result : INVALID

reference_data : None

result : INVALID

### ProductLoad

name : ProductLoad

role : Check if the product information has been retrieved correctly

#### information

WARNING : Substances without CAS or EC numbers are omitted

#### missing_codes

reference_data : None

result : UNKNOWN

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

No information available

#### missing_codes

reference_data : None

result : NOT_AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

signal_word :

#### missing_codes

reference_data : None

result : NOT_AVAILABLE

### Precautionary

name : Precautionary

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

No information available

#### missing_codes

reference_data : None

result : NOT_AVAILABLE

### PCode

name : PCode

role : Check if the P-codes of a product are valid based on its H-codes

#### information

Reference Codes :

Actual Codes :

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

reference_data : None

result : VALID

### Classification

name : Classification

role : Check the classification of a product based on its pH and substances concentrations

#### information

reason : Si une substance a une classification H340 et est présente à une concentration >= 0,1 %, le produit doit être classé H340 (Mutagène).

substance_name : Naphta léger (pétrole), hydrotraité

substance_classification : H340

substance_concentration : None–10.0%

rule_threshold : 0.1%

classification : Le produit doit avoir la classification supplémentaire ['H340'].

reason : Si une substance a une classification H350 et est présente à une concentration >= 0,1 %, le produit doit être classé H350 (Cancérogène).

substance_name : Naphta léger (pétrole), hydrotraité

substance_classification : H350

substance_concentration : None–10.0%

rule_threshold : 0.1%

classification : Le produit doit avoir la classification supplémentaire ['H350'].

#### missing_codes

H340, H350

reference_data : None

result : INVALID

## Butane

cas : 106-97-8

name : Butane

### h_codes

H220, H280

concentrations : greater or equal to 60.0 and less or equal to 90.0

ec : None

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H220

Actual Codes : H220, H280

Codes in both sets : H220

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

vle-courte-ppm : 980.0

vle-courte-mg-m3 : 2370.0

#### missing_codes

result : REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Butane

h_code : H220

###### categories

code : P2

section : P

label : P2 GAZ INFLAMMABLES Gaz inflammables, catégorie 1 ou 2

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H220 : code: H220 exposition: danger: Flam. Gas text: Gaz extrêmement inflammable.

H280 : code: H280 exposition: danger: Label elements for gases under pressure text: Contient un gaz sous pression; peut exploser sous l’effet de la chaleur.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS04, GHS02

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Butane

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Poly(diméthylsiloxane)

cas : 63148-62-9

name : Poly(diméthylsiloxane)

### h_codes

concentrations : greater or equal to 5.0 and less or equal to 20.0

ec : None

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes :

Actual Codes :

Codes in both sets :

reason : The result is valid because all codes from the reference data are found in the actual data

#### missing_codes

result : VALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

No information available

#### missing_codes

result : NOT_AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

signal_word :

#### missing_codes

result : NOT_AVAILABLE

### INRS

name : INRS

#### information

WARNING : No INRS data found for Poly(diméthylsiloxane)

#### missing_codes

result : NOT_AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

## Naphta léger (pétrole), hydrotraité

cas : 64742-49-0

name : Naphta léger (pétrole), hydrotraité

### h_codes

H225, H304, H315, H336, H340, H350

concentrations : strictly less than 10.0

ec : None

## Validations

### HazardStatement

name : HazardStatement

role : Check if the H-codes of a substance are valid based on its CAS number by comparing them to a reference data set from ECHA CLH

#### information

Reference Codes : H304, H340, H350

Actual Codes : H225, H304, H315, H336

Codes in both sets : H304

reason : The result is invalid because there are codes in the reference data but not in the actual data

Missing Codes : H340, H350

WARNING : Added Missing Codes ['H340', 'H350'] to Naphta léger (pétrole), hydrotraité

###### New codes are now

H225, H304, H315, H336, H340, H350

#### missing_codes

H340, H350

result : INVALID

### POP

name : POP

role : Check if the product must be compliant with the POP regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### REACH

name : REACH

role : Check if the product must be compliant with the REACH regulations according to REACH Annex XVII and XIV

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### COBET

name : COBET

role : Check if the product must be compliant with the COBET regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### RPB

name : RPB

role : Check if the product must be compliant with the RPB regulations

#### information

No information available

#### missing_codes

result : NOT_REGULATED

### SEVESO

name : SEVESO

role : Check if the product must be compliant with the CEVESO regulations

#### information

regulation : SEVESO

substance : Naphta léger (pétrole), hydrotraité

h_code : H225

###### categories

code : P5a

section : P

label : P5a LIQUIDES INFLAMMABLES — Liquides inflammables, catégorie 1, ou — liquides inflammables de catégorie 2 ou 3, maintenus à une température supérieure à leur point d'ébullition, ou — autres liquides dont le point d'éclair est inférieur ou égal à 60 °C, maintenus à une température supérieure à leur point d'ébullition (voir note 12)

threshold_low : 10.0

threshold_high : 50.0

unit : tonnes

code : P5b

section : P

label : P5b LIQUIDES INFLAMMABLES — Liquides inflammables de catégorie 2 ou 3 dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs, ou — autres liquides ayant un point d'éclair inférieur ou égal à 60 °C, dont les conditions particulières de traitement, telles qu'une pression ou une température élevée, peuvent représenter des dangers d'accidents majeurs (voir note 12)

threshold_low : 50.0

threshold_high : 200.0

unit : tonnes

code : P5c

section : P

label : P5c LIQUIDES INFLAMMABLES Liquides inflammables de catégorie 2 ou 3 non couverts par les catégories P5a et P5b

threshold_low : 5000.0

threshold_high : 50000.0

unit : tonnes

#### missing_codes

result : REGULATED

### Exposure

name : Exposure

role : Checks the Substance exposure and labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

H225 : code: H225 exposition: danger: Label elements for flammable liquids text: Liquide et vapeurs très inflammables.

H304 : code: H304 exposition: danger: Asp. Tox. text: Peut être mortel en cas d’ingestion et de pénétration dans les voies respiratoires.

H315 : code: H315 exposition: danger: 3.2.4.

Hazard Communication text: Provoque une irritation cutanée.

H336 : code: H336 exposition: danger: Label elements for specific target organ toxicity after single exposure text: Peut provoquer somnolence ou vertiges.

H340 : code: H340 exposition: danger: Muta. text: Peut induire des anomalies génétiques.

H350 : code: H350 exposition: danger: Carc. text: Peut provoquer le cancer.

#### missing_codes

result : AVAILABLE

### Labeling

name : Labeling

role : Checks the Substance labeling data. see https://echa.europa.eu/documents/10162/2324906/clp_labelling_en.pdf/89628d94-573a-4024-86cc-0b4052a74d65 see https://echa.europa.eu/regulations/clp/clp-pictograms

#### information

###### pictograms

GHS08

signal_word : Danger

#### missing_codes

result : AVAILABLE

### INRS

name : INRS

#### information

fiche : Fiche n°322 - Solvants aliphatiques en C5-C9

url : https://www.inrs.fr/publications/bdd/fichetox/fiche.html?refINRS=FICHETOX_322

###### sections

Généralités, Caractéristiques, VLEPMesurage, Incendie - Explosion[10-12], Pathologie - Toxicologie, Règlementation, Recommandations, Bibliographie

#### missing_codes

result : AVAILABLE

role : None

### CMR

name : CMR

role : Check if the product must be compliant with the CMR regulations

#### information

regulation : CMR

substance : Naphta léger (pétrole), hydrotraité

h_code : H340

regulation : CMR

substance : Naphta léger (pétrole), hydrotraité

h_code : H350

#### missing_codes

result : REGULATED